**Beacon and Lightbar fitting/use information**

This information is applicable to the UK only.

All warning beacons/lightbars should be mounted on the vehicle so that the centre of the lamp is no less than 1200mm above the ground.

The beacon/lightbar base should be parallel with the ground and fitted to the flattest part of the vehicle roof on a central line across the vehicle.

The light from the beacon/lightbar should be visible from any point at a reasonable distance from the vehicle or any trailer being towed by a vehicle.

AMBER is the only permitted colour in the UK unless used on an emergency service vehicle (BLUE) or by a registered GMC medical practioner (Green)

When fitting a beacon/lightbar to a vehicle with radio equipment, the distance to the aerial should not be less than 500mm.

It is good practice to route product supply cables away from sensitive cables eg.radio, aerials, anti-lock braking systems etc. If this is not possible cross cables at right angles.

Disconnect from battery before wiring up.Bottom of Form

Bottom of Form