RELAY CONFIGURATIONS

 **Relays – Connecting & Clamping**

 German Iso 7588 Description

 Standard Standard

 86 1 Coil Trigger (+)

 85 2 Coil Trigger (-)

 Ground

 30 3 Battery (+)

 87a 4 Output 2

 87 5 Output 1



