RELAY CONFIGURATIONS

**Relays – Connecting & Clamping**

German Iso 7588 Description

Standard Standard

86 1 Coil Trigger (+)

85 2 Coil Trigger (-)

Ground

30 3 Battery (+)

87a 4 Output 2

87 5 Output 1



